****

 **TECHNINIŲ PARAMETRŲ LAPAS**

 **Konverteris DC/DC**

**P 2x 1k2 6-60/12-80 IP65**



**Maitinimo įtampa [PRI]:]: 2x 6÷60V DC**

**Ramybės srovė: 2x 15mA**

**Įvesties srovė [Imax]: 2x 20A**

**Maksimalios apkrovos srovė [Imax]: 2x 20A**

**Reguliuojama išėjimo įtampa**  **[SEC]: 2x 12÷80V DC**

**Išėjimo galia: [P] 2x 1200W**

**Darbinė temperatūra [ta] -45oC÷85oC**

**Efektyvumas: >95%**

**Matmenys: 201/163/98 mm**

**Svoris: ≈ 3kg**

**Korpusas konverteris DC/DC P 1k2 6-60/12-80 IP65**

|  |
| --- |
|  |
|

|  |
| --- |
| **Matmenys** |
| Width [B](mm): | 163 |
| Height [A](mm):  | 201 |
| Depth [h] (mm): | 99 |
| Weight (kg): | 1 |

 |  |
| **Technical parameters** |
| Degree of protection IP : | IP 65 |
| Mechanical endurance IK : | IK 07 |
| Electric isolation: | Complete isolation (II) |
| Class of flammability : | UL 94 HB |
| Test of glowing-hot wire °C: | 650 |
| **Materials** |
| Material: | ABS |
| The colour of basis: | RAL 7035 |
| The colour of cover: | RAL 7035 |
| The material of screws to covers: | Poliamid |
| The colour of screws to covers: | Gray |
| The material of gasket: | PUR |
| **Darbinė temperatūra** |
| Min temp °C (a short time): | -40 |
| Max temp °C (a short time): | 80 |
| Min temp °C (continuous work): | -40 |
| Max temp °C (continuous work): | 60 |

